|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | ASIA-PACIFIC TELECOMMUNITY |  | |  |
| **APT Coordination Meetings During RA-12 and WRC-12** | |  | |
|  | |  | |

Date: 2012/01/31

**REPORT OF THE WRC-12 AGENDA ITEM COORDINATOR**

|  |
| --- |
| **Agenda Item No.**: Agenda item 1.18 |
| **Name of the Coordinator ( with Email)**: Zhao xiaodong (CHN),  Emai : xiaodongzhao1963@vip.sina.com |
| **Issues:**  to consider extending the existing primary and secondary radiodetermination-satellite service (space-to-Earth) allocations in the band 2 483.5-2 500 MHz in order to make a global primary allocation, and to determine the necessary regulatory provisions based upon the results of ITU‑R studies, in accordance with Resolution **613 (WRC‑07)**; |
| **APT Proposals**:  APT Members support extending the existing primary and secondary radiodetermination-satellite service (space-to-Earth) allocations in the band 2 483.5-2 500 MHz to make a global primary allocation on the following proposals below.   1. Modify the footnote 5.400:   5.400 In Angola, Australia, Bangladesh, Burundi, China, Eritrea, Ethiopia, India, Iran (Islamic Republic of), the Libyan Arab Jamahiriya, Lebanon, Liberia, Madagascar, Mali, Pakistan, Papua New Guinea, the Dem. Rep. of the Congo, the Syrian Arab Republic, Sudan, Swaziland, Togo and Zambia, the use of RDSS systems for which their complete coordination information has been received by the Radiocommunication Bureau before [the end of WRC‑12], while retaining the primary status that they had before WRC‑12, shall continue to apply the procedure of No. **9.21** with respect to the countries not listed in this footnote (see also the provisions of No. **7.4A**).     (WRC‑12)  **Reasons:** These provisions will retain the regulatory status of the existing RDSS systems after the global upgrade allocation in this band.   1. To keep the threshold values of MSS and RDSS no change in appendix 5. |
| **Status of the APT Proposals:** |
| **Issues to be discussed at the Coordination Meeting:**  PFD level  **Keep the MSS and RDSS PFD no change.** |
| **Comments/Remarks by the Coordinator**:   1. The MSS threshold value increase issue: the APT position is no change. please pay more attention to this issue. |